<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="36" y2="52" width="0" layer="20"/>
<wire x1="36" y1="52" x2="0" y2="52" width="0" layer="20"/>
<wire x1="0" y1="52" x2="0" y2="0" width="0" layer="20"/>
<circle x="3" y="4" radius="1.6" width="0.1524" layer="20"/>
<text>12V</text>
<text>TX</text>
<text>RX</text>
<text>GND</text>
<text>ON/OFF</text>
<text>SILENT</text>
<text>MAIANA™ AIS
Breakout
Rev. 3.0</text>
<circle x="33" y="33" radius="1.6" width="0.1524" layer="20"/>
<text>+</text>
<text>-</text>
</plain>
<libraries>
<library name="MyPassives">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="e-switch">
<packages>
<package name="LC1258XXNP">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diodesinc">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="MyDiodes">
<packages>
<package name="SMB-BIDIR">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="ost-2pin-contact">
<packages>
<package name="CONN_OSTVN02A150_OST">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20R">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="v-reg-micrel">
<description>&lt;b&gt;Micrel Voltage Regulator&lt;/b&gt;&lt;p&gt;
Micrel Semiconductor, Inc.&lt;br&gt;
http://www.micrel.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
<variantdef name="NO_NMEA"/>
</variantdefs>
<elements>
<element name="GPS" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ON_OFF" library="e-switch" package="LC1258XXNP" value="LC1258EENP">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="DMP3099L-7">
<attribute name="VALUE"/>
</element>
<element name="R1" library="MyPassives" package="0603" value="10k">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="MyPassives" package="0603" value="2k2">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="MyPassives" package="0603" value="2k2">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="MyPassives" package="0603" value="2k2">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="MyPassives" package="0603" value="2k2">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SILENT" library="e-switch" package="LC1258XXNP" value="LC1258EENP">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="diodesinc" package="SOT23-6" value="DMG6602SVT">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="RJ45-8" value="54602-908LF">
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="D1" library="MyDiodes" package="SMB-BIDIR" value="SMBJ16CA">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="adafruit" package="R1206" value="BSMD1206-050-16V">
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="DMP3099L-7">
<attribute name="VALUE"/>
</element>
<element name="J1" library="ost-2pin-contact" package="CONN_OSTVN02A150_OST" value="OSTVN02A150">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="OSTVN02A150"/>
<attribute name="SOURCELIBRARY" value="On_Shore_Technology_2019-12-02"/>
<attribute name="VENDOR" value="On Shore Technology Inc"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0603-CAP" value=".1uF">
<attribute name="PARTNO" value="GRM188R71E223KA01D"/>
<attribute name="VALUE"/>
</element>
<element name="TX_OFF" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GPS_STAT" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="RX_EVT" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="V_IN" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="V_CTRL" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="TX_EVT" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="V_OUT" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="12V" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND1" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND2" library="testpad" package="TP20R" value="TPTP20R">
<attribute name="NAME"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="IC1" library="v-reg-micrel" package="SOT23-5" value="MIC5203-3.3YM5-TR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="MyPassives" package="0603" value="1uF">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="MyPassives" package="0603" value="1uF">
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="1X04" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q1" pad="1"/>
<contactref element="R2" pad="P$2"/>
<contactref element="JP2" pad="8"/>
<contactref element="D1" pad="C"/>
<contactref element="U3" pad="5"/>
<contactref element="TX" pad="C"/>
<contactref element="J1" pad="1"/>
<contactref element="C8" pad="2"/>
<contactref element="GND1" pad="TP"/>
<contactref element="GND2" pad="TP"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="SILENT" pad="P$1"/>
<contactref element="ON_OFF" pad="P$1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="12V">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="12V" pad="TP"/>
</signal>
<signal name="V_IN">
<contactref element="Q1" pad="2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U3" pad="2"/>
<contactref element="ON_OFF" pad="P$3"/>
<contactref element="V_IN" pad="TP"/>
</signal>
<signal name="V_OUT">
<contactref element="JP2" pad="1"/>
<contactref element="F1" pad="2"/>
<contactref element="V_OUT" pad="TP"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="P$1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="TX_DISABLE">
<contactref element="SILENT" pad="P$2"/>
<contactref element="JP2" pad="2"/>
<contactref element="Q2" pad="1"/>
<contactref element="TX_OFF" pad="TP"/>
</signal>
<signal name="GPS_STATUS">
<contactref element="R3" pad="P$2"/>
<contactref element="JP2" pad="4"/>
<contactref element="GPS_STAT" pad="TP"/>
</signal>
<signal name="AIS_RX_EVENT">
<contactref element="R4" pad="P$2"/>
<contactref element="JP2" pad="6"/>
<contactref element="RX_EVT" pad="TP"/>
</signal>
<signal name="AIS_TX_EVENT">
<contactref element="JP2" pad="7"/>
<contactref element="TX" pad="A"/>
<contactref element="R5" pad="P$2"/>
<contactref element="TX_EVT" pad="TP"/>
</signal>
<signal name="3.3V">
<contactref element="GPS" pad="A"/>
<contactref element="RX" pad="A"/>
<contactref element="SILENT" pad="P$3"/>
<contactref element="PWR" pad="A"/>
<contactref element="Q2" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="P$1"/>
<contactref element="U3" pad="6"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="PWR_CTRL">
<contactref element="U3" pad="1"/>
<contactref element="V_CTRL" pad="TP"/>
<contactref element="ON_OFF" pad="P$2"/>
</signal>
<signal name="N$2">
<contactref element="PWR" pad="C"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="GPS" pad="C"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="RX" pad="C"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="TRANSPONDER_UART_TX">
<contactref element="JP2" pad="5"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="TRANSPONDER_UART_RX">
<contactref element="JP2" pad="3"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U3" pad="4"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="P$1"/>
<contactref element="Q2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
