<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="55.86" y2="0" width="0" layer="20"/>
<wire x1="55.86" y1="0" x2="55.86" y2="17.45" width="0" layer="20"/>
<wire x1="55.86" y1="17.45" x2="0" y2="17.45" width="0" layer="20"/>
<wire x1="0" y1="17.45" x2="0" y2="0" width="0" layer="20"/>
<text>MAIANA(TM)
UART Breakout v2.0
(c)2021 P.Antypas</text>
<circle x="38.1" y="14.5" radius="1.1" width="0.0762" layer="20"/>
<circle x="2.3" y="2.3" radius="1.1" width="0.0762" layer="20"/>
<text>RX_LED</text>
<text>GPS_LED</text>
<text>UART_RX</text>
<text>UART_TX</text>
<text>TX_OFF</text>
<text>9-18V</text>
<text>TX_LED</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>GND</text>
<text>GND</text>
<text>3.3V</text>
<text>3.3V</text>
<text>3.3V</text>
<text>GND</text>
</plain>
<libraries>
<library name="MyPassives">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="MyDiodes">
<packages>
<package name="SMB-BIDIR">
</package>
<package name="SOD123">
<description>SOD123 Package</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ45-8">
</package>
<package name="1X08">
</package>
</packages>
</library>
<library name="microchip">
<description>&lt;b&gt;Microchip PIC Microcontrollers and other Devices&lt;/b&gt;&lt;p&gt;
Based on the following sources :
&lt;ul&gt;
&lt;li&gt;Microchip Data Book, 1993
&lt;li&gt;THE EMERGING WORLD STANDARD, 1995/1996
&lt;li&gt;Microchip, Technical Library CD-ROM, June 1998
&lt;li&gt;www.microchip.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
<variantdef name="JLCPCB"/>
</variantdefs>
<elements>
<element name="C1" library="MyPassives" package="0603" value="1uF">
<attribute name="PARTNO" value="CC0603KRX5R8BB105"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="MyPassives" package="0603" value="1uF">
<attribute name="PARTNO" value="CC0603KRX5R8BB105"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="MyDiodes" package="SMB-BIDIR" value="SMBJ14CA">
<attribute name="PARTNO" value="SMBJ14CA"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="MyDiodes" package="SOD123" value="WSB5508L-2/TR">
<attribute name="PARTNO" value="WSB5508L-2/TR"/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="adafruit" package="R1206" value="BSMD1206-050-16V">
<attribute name="PARTNO" value="BSMD1206-050-16V"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="RJ45-8" value="95501-2821">
<attribute name="PARTNO" value="95501-2821"/>
<attribute name="PROD_ID" value="CONN-08506"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="microchip" package="SOT23" value="SE8533X2-HF">
<attribute name="PARTNO" value="SE8533X2-HF"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J2" pad="8"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="U1" pad="1"/>
<contactref element="JP2" pad="4"/>
<contactref element="JP3" pad="4"/>
<contactref element="JP3" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="TRANSPONDER_UART_TX">
<contactref element="J2" pad="5"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="12V">
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="A"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="TX_OFF">
<contactref element="J2" pad="2"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="GPS_LED">
<contactref element="J2" pad="4"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="RX_LED">
<contactref element="J2" pad="6"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="TX_LED">
<contactref element="J2" pad="7"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="V_IN">
<contactref element="F1" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="TRANSPONDER_UART_RX">
<contactref element="J2" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="V_OUT">
<contactref element="F1" pad="2"/>
<contactref element="C1" pad="P$1"/>
<contactref element="U1" pad="3"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="C2" pad="P$1"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="JP3" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
