<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="5" y1="2" x2="0" y2="5.9" width="0.001" layer="20" curve="104.478019"/>
<wire x1="0" y1="40.1" x2="5" y2="44" width="0.001" layer="20" curve="104.477998"/>
<wire x1="4.5" y1="0" x2="5" y2="2" width="0.001" layer="20" curve="30.000012"/>
<wire x1="5" y1="44" x2="4.5" y2="46" width="0.001" layer="20" curve="30.000012"/>
<circle x="3" y="10" radius="0.8" width="0.001" layer="20"/>
<wire x1="0" y1="40.1" x2="5" y2="44" width="0.001" layer="20" curve="104.477998"/>
<wire x1="0" y1="40.1" x2="5" y2="44" width="0.001" layer="20" curve="104.477998"/>
<wire x1="0" y1="5.9" x2="0" y2="40.1" width="0.001" layer="20"/>
<wire x1="5" y1="2" x2="0" y2="5.9" width="0.001" layer="20" curve="104.478019"/>
<wire x1="0" y1="40.1" x2="5" y2="44" width="0.001" layer="20" curve="104.477998"/>
<wire x1="4.5" y1="0" x2="5" y2="2" width="0.001" layer="20" curve="30.000012"/>
<wire x1="5" y1="44" x2="4.5" y2="46" width="0.001" layer="20" curve="30.000012"/>
<circle x="3" y="10" radius="0.8" width="0.001" layer="20"/>
<wire x1="5" y1="2" x2="0" y2="5.9" width="0.001" layer="20" curve="104.478019"/>
<wire x1="5" y1="2" x2="0" y2="5.9" width="0.001" layer="20" curve="104.478019"/>
<wire x1="4.5" y1="0" x2="5" y2="2" width="0.001" layer="20" curve="30.000012"/>
<wire x1="4.5" y1="0" x2="5" y2="2" width="0.001" layer="20" curve="30.000012"/>
<wire x1="5" y1="44" x2="4.5" y2="46" width="0.001" layer="20" curve="30.000012"/>
<wire x1="5" y1="44" x2="4.5" y2="46" width="0.001" layer="20" curve="30.000012"/>
<wire x1="4.5" y1="0" x2="31.5" y2="0" width="0.001" layer="20"/>
<wire x1="4.5" y1="46" x2="31.6" y2="46" width="0.001" layer="20"/>
<wire x1="36" y1="5.9" x2="31.5" y2="0" width="0.001" layer="20" curve="134.477531"/>
<wire x1="31.6" y1="46" x2="36" y2="40.1" width="0.001" layer="20" curve="134.477531"/>
<wire x1="36" y1="5.9" x2="36" y2="40.1" width="0.001" layer="20"/>
<circle x="3" y="10" radius="0.8" width="0.001" layer="20"/>
<circle x="3" y="10" radius="0.8" width="0.001" layer="20"/>
<circle x="33" y="36" radius="0.8" width="0.001" layer="20"/>
<text>+</text>
<text>-</text>
<text>MAIANA USBControl Box
Rev 2.0</text>
</plain>
<libraries>
<library name="transistor-small-signal">
<description>&lt;b&gt;Small Signal Transistors&lt;/b&gt;&lt;p&gt;
Packages from :&lt;br&gt;
www.infineon.com; &lt;br&gt;
www.semiconductors.com;&lt;br&gt;
www.irf.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MyPassives">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="MyDiodes">
<packages>
<package name="SMB-BIDIR">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="ost-2pin-contact">
<packages>
<package name="CONN_OSTVN02A150_OST">
</package>
</packages>
</library>
<library name="v-reg-micrel">
<description>&lt;b&gt;Micrel Voltage Regulator&lt;/b&gt;&lt;p&gt;
Micrel Semiconductor, Inc.&lt;br&gt;
http://www.micrel.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="JiangsuQinHeng">
<packages>
<package name="SOIC-8">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="yenji">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="10118194-0001LF">
<packages>
<package name="AMPHENOL_10118194-0001LF">
</package>
</packages>
</library>
<library name="xyfw">
<packages>
<package name="RJ-82A86MMNL">
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="CL-SB-12B-01T">
<packages>
<package name="CL-SB-12B">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
<variantdef name="JLCPCB"/>
</variantdefs>
<elements>
<element name="Q1" library="transistor-small-signal" package="SOT23" value="DMP3099L-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="MyPassives" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="MyDiodes" package="SMB-BIDIR" value="SMBJ16CA">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="F1" library="adafruit" package="R1206" value="BSMD1206-050-16V">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="ost-2pin-contact" package="CONN_OSTVN02A150_OST" value="OSTVN02A150">
<attribute name="BUILT_BY" value="EMA_Cory"/>
<attribute name="COPYRIGHT" value="Copyright (C) 2018 Accelerated Designs. All rights reserved"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="OSTVN02A150"/>
<attribute name="SOURCELIBRARY" value="On_Shore_Technology_2019-12-02"/>
<attribute name="VALUE"/>
<attribute name="VENDOR" value="On Shore Technology Inc"/>
</element>
<element name="IC1" library="v-reg-micrel" package="SOT23-5" value="MIC5203-3.3YM5-TR">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="MyPassives" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="MyPassives" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="transistor-small-signal" package="SOT23" value="DMP3099L-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="adafruit" package="SOT23" value="BSS138">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="JiangsuQinHeng" package="SOIC-8" value="CH340N">
<attribute name="NAME"/>
<attribute name="PARTNO" value="CH340N"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="MyPassives" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="MyPassives" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="MyPassives" package="0603" value="75R">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SOD-323" value="3.3V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-11284"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="yenji" package="SOT23-6" value="SRV05-4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="10118194-0001LF" package="AMPHENOL_10118194-0001LF" value="10118194-0001LF">
<attribute name="ARROW_ELECTRONICS-PURCHASE-URL" value="https://snapeda.com/shop?store=Arrow+Electronics&amp;id=4816633"/>
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="DESCRIPTION" value=" USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle; Through Hole "/>
<attribute name="DIGIKEY-PURCHASE-URL" value="https://snapeda.com/shop?store=DigiKey&amp;id=4816633"/>
<attribute name="MF" value="Amphenol ICC (FCI)"/>
<attribute name="MOUSER-PURCHASE-URL" value="https://snapeda.com/shop?store=Mouser&amp;id=4816633"/>
<attribute name="MP" value="10118194-0001LF"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="xyfw" package="RJ-82A86MMNL" value="RJ-82A86MMNL">
<attribute name="NAME"/>
<attribute name="PARTNO" value="RJ-82A86MMNL"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="TJ-S3216CL9T5ALC2G-A5"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="MyPassives" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="DMP3099L-7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="TJ-S3216CL9T5ALC2G-A5"/>
<attribute name="VALUE"/>
</element>
<element name="GPS" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="TJ-S3216CL9T5ALC2G-A5"/>
<attribute name="VALUE"/>
</element>
<element name="PWR" library="led" package="CHIPLED_1206" value="">
<attribute name="NAME"/>
<attribute name="PARTNO" value="TJ-S3216CL9T5ALC2G-A5"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="MyPassives" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="MyPassives" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="MyPassives" package="0603" value="2k2">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="SILENT" library="CL-SB-12B-01T" package="CL-SB-12B" value="CL-SB-12B-01T">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Slide Switch SPDT Surface Mount "/>
<attribute name="MF" value="Nidec Copal"/>
<attribute name="MP" value="CL-SB-12B-01T"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="ON_OFF" library="CL-SB-12B-01T" package="CL-SB-12B" value="CL-SB-12B-01T">
<attribute name="AVAILABILITY" value="In Stock"/>
<attribute name="DESCRIPTION" value=" Slide Switch SPDT Surface Mount "/>
<attribute name="MF" value="Nidec Copal"/>
<attribute name="MP" value="CL-SB-12B-01T"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="R7" library="MyPassives" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="MyPassives" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="MyPassives" package="0603" value="1uF">
<attribute name="NAME"/>
<attribute name="PARTNO" value=""/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="2"/>
<contactref element="Q1" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="Q4" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C4" pad="P$2"/>
<contactref element="C5" pad="P$2"/>
<contactref element="D2" pad="A"/>
<contactref element="U$4" pad="2"/>
<contactref element="J2" pad="S3"/>
<contactref element="J2" pad="S1"/>
<contactref element="J2" pad="S4"/>
<contactref element="J2" pad="S2"/>
<contactref element="J2" pad="S5"/>
<contactref element="J2" pad="S6"/>
<contactref element="J3" pad="P$8"/>
<contactref element="J3" pad="P$11"/>
<contactref element="J3" pad="P$9"/>
<contactref element="J3" pad="P$12"/>
<contactref element="J3" pad="P$10"/>
<contactref element="TX" pad="C"/>
<contactref element="R2" pad="P$2"/>
<contactref element="ON_OFF" pad="1"/>
<contactref element="R7" pad="P$2"/>
<contactref element="J2" pad="5"/>
<contactref element="SILENT" pad="3"/>
<contactref element="C3" pad="P$2"/>
</signal>
<signal name="TRANSPONDER_UART_TX">
<contactref element="U$1" pad="7"/>
<contactref element="J3" pad="P$5"/>
</signal>
<signal name="TRANSPONDER_UART_RX">
<contactref element="U$1" pad="6"/>
<contactref element="J3" pad="P$3"/>
</signal>
<signal name="12V">
<contactref element="Q1" pad="3"/>
<contactref element="D1" pad="A"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="V_OUT">
<contactref element="F1" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="P$1"/>
<contactref element="J3" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="R1" pad="P$1"/>
<contactref element="Q3" pad="1"/>
<contactref element="Q4" pad="3"/>
</signal>
<signal name="PWR_CTRL">
<contactref element="Q4" pad="1"/>
<contactref element="ON_OFF" pad="2"/>
<contactref element="R7" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="F1" pad="1"/>
<contactref element="Q3" pad="3"/>
</signal>
<signal name="3.3V">
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="P$1"/>
<contactref element="Q2" pad="2"/>
<contactref element="GPS" pad="A"/>
<contactref element="RX" pad="A"/>
<contactref element="PWR" pad="A"/>
<contactref element="SILENT" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="8"/>
<contactref element="C4" pad="P$1"/>
</signal>
<signal name="N$12">
<contactref element="U$1" pad="5"/>
<contactref element="C5" pad="P$1"/>
<contactref element="R8" pad="P$2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="VBUS">
<contactref element="R8" pad="P$1"/>
<contactref element="U$4" pad="5"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="D-">
<contactref element="U$1" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="D+">
<contactref element="U$1" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="U$4" pad="6"/>
</signal>
<signal name="TX_DISABLE">
<contactref element="J3" pad="P$2"/>
<contactref element="Q2" pad="1"/>
<contactref element="R6" pad="P$2"/>
<contactref element="C3" pad="P$1"/>
</signal>
<signal name="GPS_STATUS">
<contactref element="J3" pad="P$4"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="AIS_RX_EVENT">
<contactref element="J3" pad="P$6"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="AIS_TX_EVENT">
<contactref element="J3" pad="P$7"/>
<contactref element="TX" pad="A"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="P$1"/>
<contactref element="Q2" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="PWR" pad="C"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="GPS" pad="C"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$4">
<contactref element="RX" pad="C"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="V_IN">
<contactref element="ON_OFF" pad="3"/>
<contactref element="R1" pad="P$2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="SILENT" pad="2"/>
<contactref element="R6" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
